

USB CAN module use gs\_usb.ko driver along with official Linux kernel , enable gs\_usb driver


In kernel menuconfig and install the gs\_usb.ko to your system.


Kernel config :














And then make the kernel,Please refer to the build kernel method on different platform

Raspberry Pi 4:

make ARCH=arm CROSS\_COMPILE=arm-linux-gnueabihf- zImage modules dtbs -j4